Comandos útiles para Raspberry Pi

# Reiniciar Mosquitto

sudo systemctl restart mosquitto

# Reiniciar OpenHab

sudo systemctl restart openhab2.service

# Conectar a la consola de OpenHab

ssh -p 8101 openhab@localhost

# Abrir la configuración de OpenHabian

sudo openhabian-config