Comandos útiles para Raspberry Pi

# Reiniciar Mosquitto

sudo systemctl restart mosquitto

# Conectar a la consola de OpenHab

ssh -p 8101 openhab@localhost